Trimble PivotTM Platform, version 2.1.5
This patch for Trimble Pivot Platform contains all changes since version 2.1.0. The following document gives you an overview about the changes. 

DCB File reader
The DCB File reader has been adapted to reflect changes in PRN numbering introduced by the CODE analysis center. 

NTRIP Caster – Access Server Support
The Trimble NTRIP Caster now supports the Cisco Access Server 2900 Series in addition. The NTRIP Caster properties now offer a field to select the correct Access Server series. When updating the software, the default setting is the 5300 / 5400 series. 

Post processing engine
The processing algorithms within the post processing engine have been improved.

RINEX storage – Hatanaka compression
The Hatanaka compression within the RINEX storage module has been improved to provide a complete Hatanaka file when re-starting a server during an hour. A system restart could cause the loss of data for the session prior to the start.

RTO module
The RTCM3 generation has been changed to no longer allow “special characters” like ü for station names. In case of the usage of “special characters” in your station name, this character will be replaced by underscore (_) when sending out RTCM3 messages.

Trimble PivotTM Platform, version 2.1.3
Trimble NTRIP Caster Access Server Connection
When a user connects through GSM into the software through an Access Server, it might appear a user is being disconnected from the system. The Pivot Patch is now preventing the user from automatically being disconnected.

Trimble Reference Data Shop
The Reference Data Shop is now supporting T02 file import of station data containing a combination of letters and numbers for the station code. 

RTO DGPS Output
Improved satellite data output from RTO DGPS module.

Trimble Pivot™ Platform, version 2.1.2
DBServer redundancy handling
The DBServer has been improved to keep active sessions open from the running DBServer in case you need to restart one of the DBServers. This applies to a redundant system with one common accounting data base. This improvement requires a new DBServer ID, which needs to be configured manually. Please contact Infrastructure_Support@Trimble.com for further information, in case you are running a redundant setup with a common accounting data base.

Ephemeris Download
The ephemeris download module is now offering a new property, which allows selecting between a passive or an active FTP download for predicted orbits and DCB files. The default setting is passive.

Post Processing Engine
The interval handling for kinematic sessions in the post processing engine has been improved.

RTX-PP Engine
The default session interval for the RTX-PP engine has been changed from 1 hour to 24 hours.

Session report
The session recording has now been improved to always show the correct epochs for the full amount in the session reports. Previously, in cases where a customer was working at the same time his subscription was being terminated, the information on the full amount in the session report may show an incorrect number, while the effective amount always showed the correct information about the used time. 
Note: This change is based on a change in the accounting data base. In case of a redundant system with a common accounting data base, Trimble strongly recommends to apply the patch on both systems at the same time. Please make sure, that both systems are stopped, while applying the patch.