Trimble PivotTM Platform, version 2.5.2
This patch for Trimble Pivot Platform contains all changes since version 2.5.0. The following document gives you an overview about the changes. 

GNSS receiver module
Pivot 2.1 offered CMRx as input decoder type within the GNSS receiver module. By  accident, this functionality did not show up in Pivot 2.5. The input decoder type CMRx for NetR5, NetR8 and NetR9 is now available again.

RTO module – 
LLI handling in CMR+ data streams
The LLI (Loss of Lock Indicator) did not increase while switching a master station within a VRS data stream. The RTO module has been improved to now provide correct LLI handling for moving rovers using CMR+ correction data.
NMEA strings from GSM connections
RTO module has been improved to correctly read NMEA strings submitted during a GSM dial in connection, even if this information is submitted in multiple data packages.

Trimble PivotTM Platform, version 2.5.1
DBServer improvement in redundant setup
When two active sessions in a redundant system with two DBServers accessing a common accounting data base are ended simultaneously, it can happen that one session remains open until the respective DBServer can be restarted. This may result in incorrect end time. The end session handling for redundant systems has now been improved to avoid such behavior.

iGate module
The iGate module has been improved to better handle the communication to office software products like Trimble Business Center and Trimble Pathfinder Office software in case of a slow connection between the office computer and the server system.