Trimble PivotTM Platform, version 3.10.3 
This software update for Trimble® Pivot™ Platform (TPP) contains all changes since the release of version 3.10.0. The following document gives you an overview of the changes.
Software update version 3.10.3 contains identical content as previous version 3.10.2. Version 3.10.2 has been withdrawn from the automatic update mechanism due to an unexpected issue with high station delays that might have affected some networks. This issue has been fixed and version 3.10.2 gets re-released as version 3.10.3. 

Trimble PivotTM Platform, version 3.10.2
Real Time Output
RTO Performance
In case a rover’s associated Physical Base Station changed while the rover is connected, the rover performance could have been limited for up to one minute. This issue has been fixed.
RTO with Sub-networks
Improved the sub-network selection when rovers are connecting near the borders or within the overlapping area of two or more sub-networks.

Trimble Format Updates
NMEA GGK Message String
The GGK message is a Trimble-proprietary extension to the NMEA message which typically consists of 12 fields. Extended information may be configured, however, thus extending the number of fields for a GGK message. Trimble Pivot Platform now supports GGK strings containing more than 13 fields. 

Code Bias Calibration
Code-Bias Calibration caches station information and was lacking to clear information if a station has been moved to a new Code-Bias Calibration module. This issue could have resulted in faulty processing information. This potential issue has been fixed. 

Ephemeris Download
The Bernese GNSS Software team (Astronomical Institute of the University of Berne) has announced a change of the URL of its FTP server for predicted orbit download. The previous URL will be deactivated in September 2017. The Ephemeris Download module has been adapted to use the new address Ftp.aiub.unibe.ch.   

Ephemeris Manager
Improved internal handling of almanac storage.

Trimble Ntrip Caster
New setting for the Ntrip Server connection type when adding or editing mountpoints: An option to disconnect inactive data sources after a specified time gap of data has been added. 

Reference Data Shop
The selection of the correct epoch of network correction data has been improved. A check for the number of available satellites has been added.

Online Licensing
MAC address recognition
The recognition procedure for a changed MAC address has been improved. 
License server
Support for TLS 1.2 encryption protocol has been added for Trimble License Server.

Trimble PivotTM Platform, version 3.10.1
User Interface
Google Maps View #1
The Google Maps view might have been visible in only half of the window in version 3.8 or lower. This issue has been fixed. 
Google Maps View #2
An option has been added that allows to set “no rovers displayed” as default value in the Google Maps View properties. 
Google Maps Support in Pivot UI
Google Maps had been disabled in version 3.10. It becomes available again with this software update. For more details, please see section at the end of this document.  

Ephemeris Manager
Time-of-week has been set to wrong value in case a receiver did no longer send observation data but continued sending ephemeris information. This issue has been fixed.

Device Manager / GNSS Receiver
The way how scintillation values are displayed have changed. The respective value in the GNSS Receiver’s Raw Data Analysis view changes from numbers to none, low, medium and high. Respective scintillation filtering in the Device Manager allows selection of Off, low, medium or high. By default, scintillation filtering is turned off. 

RTXNet Processor
Master Auxiliary Concept (RTCM3Net) output
A certain setting for troposphere estimation has not been set correctly when Trimble Pivot Platform has been from version 3.8 to 3.10. This would have affected correction data output only if Master Auxiliary Concept (RTCM3Net) has been selected in a RTO referring to a RTXNet Processor. The respective setting for the troposphere estimation has been corrected with this software update. 
Residuals
Improved residuals processing and handling in RTXNet. 

Real-Time Output
Subnetwork assignment
Improved subnetwork assignment methods.
RTCM 2.3
If RTCM 2.3 and VRS were selected as correction data stream, the respective PBS coordinate has been sent out in ITRF current instead of the selected reference frame. This issue has been resolved. 

Storage
Wrong week
Week number in GPS ephemeris that is being stored in RINEX files might have been wrong. This potential issue has been resolved. 
Rinex 3.02
Galileo E1 might have been missing in the stored RINEX files. This potential issue has been resolved.  

Trimble Ntrip Caster
Mountpoint selection became case sensitive in version 3.10. It actually should not be case sensitive, this software update resolves this issue.

Code-Bias Calibration
The upload to Code-Bias Calibration with RINEX 2.x is no longer supported. Code-Bias Calibration requires RINEX 3.x or T02 files.

Trimble Accounting / Ntrip Caster
Rover users might not been able to connect to services due to concurrent sessions errors. It might have happened that users were not disconnected correctly and were not cleaned from the row SessionCount in the table ConcurrentSessions. This potential issues has been resolved.

Trimble Pivot Web
Sensor Map
The projection EPSG_9857 is replacing EPSG_900913 which will help to support WMS services. 
Missing Leap Second List / Exceptions
Several views in PIVOT Web were not able to handle time span selection in GPS time correctly. This issue has been fixed, the time span can be selected in GPS time again. 

Report Generator
Leap seconds were not handled correctly in the Report Generator if GPS time has been selected. This issue has been fixed, the reports time span can be selected in GPS time again. 

Atmo App
Weather condition
IPWV values can be stored in up to 15 seconds intervals for 24 hours before amount of data samples will be reduced to 15 minutes. 
Meteo data
The IPWV map in PIVOT Web now allows showing the following meteorological data (where available) when clicking on a station:
•	Temperature
•	Pressure
•	Humidity

Auto-Update
The Station Chart and Condition Chart for atmospheric conditions in PIVOT Web now allows setting an auto-refresh with a frequency of up to every 15 seconds. By default, auto-refresh is turned off. 

Documentation / Help files
Added missing help files for:
•	Code-Bias Calibration
•	Mobile Gate

Google Maps – New Properties
Google Maps Properties
For displaying the Google Maps view (subject to valid license for respective Pivot option), GoogleÔ requires that you register for Google Maps API Premium Plan. Refer to Google Maps APIs Premium Plan (https://developers.google.com/maps/premium/overview) for details on how to obtain a Google Maps Business license under which you may generate either a Web-API JavaScript key or a client ID. Using Google Maps in Trimble Pivot Platform requires either a Google Maps API key or a Google Maps client ID (only one can be used at a time in Trimble Pivot Platform).
New Google Maps property fields are being introduced with this software update:
•	Google Maps API key
•	Google Maps client ID
•	Automatic map update
•	Enable asset tracking

Enable asset tracking: This property specifies whether assets, such as rovers, may be tracked on the Google Maps view. By default disabled. Assets are objects which may be moving and can be tracked, such as roves in the field. For legally enabling the tracking of assets, one needs a Google Maps license that covers asset tracking. 
Show rovers: Only available, if the Enable asset tracking property is set to Yes. 

Usage limits - and how to avoid exceeding them
1) Map requests
Under the Premium Plan, customers may purchase Maps APIs Credits, that is quota for a certain period based on the estimate of the application's annual usage. All requests for Maps APIs consume credits. However, a certain quota of requests is free. At time of documentation, the following usage limits applied:
•	Shared daily free quota of 100,000 requests per 24 hours; additional requests must be paid for.  
•	For preventing abuse, the number of requests is limited to 50 requests per second.
•	The Trimble Pivot Platform Google Maps view issues one map request per view update. 

2) Asset tracking
Additional charges may arouse when the Trimble Pivot Platform Google Maps view displays the position of the rovers in the field. These moving objects are considered to be tracked assets, and as such have specific license terms and charges. 

Please note:
•	Rover states are updated every 60 seconds.
•	The Automatic map update Google Maps view-property specifies how often the map is updated.  If the property is set to Yes, the map updates once per minute which results in 1440 updates. If the property is set to No, it generates map requests only when you click the   toolbar button on top of the Google Maps view area.
•	The Enable asset tracking Google Maps view-property specifies whether assets, such as rovers, may be tracked on the Google Maps view. By default it is set to No. You should only set the property to Yes, if your Premium Plan covers asset tracking. Additionally, even if asset tracking is enabled, you may disable displaying the rovers on the map temporarily. To do so, use the Show rovers Google Maps view-property or click the  toolbar button on top of the Google Maps view area.
•	Trimble Pivot Platform internally uses the Microsoft Internet Explorer for displaying the Google Maps view. For displaying the maps correctly with the Microsoft Internet Explorer, the following web sites must be accessible for the server computer: 
*.google.com, *.gstatic.com, *.googleapis.com,  www.openstreetmap.org 
If one or several of these sites are blocked, you can add them to the list of "Trusted sites" using the Control Panel > Internet Options > Security dialog.  
•	The content of this topic refers to 3rd-party software. The methods, terms, and conditions of 3rd party software may be subject to change with or without notification. Trimble does not guarantee this content including the references to URLs to be up-to-date.