Trimble PivotTM Platform, version 3.5.4
This software update for Trimble® Pivot™ Platform (TPP) contains all changes since the release of version 3.5.0. The following document gives you an overview of the changes.

DUMMY
Trimble Online Processing App

This software update includes the release of a new App called Trimble Online Processing (TOP) App. The Trimble Online Processing App allows field users to upload rover observation data to a web-based service in order to receive post-processed positions. The final results are derived from adjusted baselines that are processed against reference stations of your local network. 
TOP is based on the Trimble Pivot Platform which provides a scalable architecture to accommodate operations ranging in size from a single base station to multi-station Real-Time Networks (RTN).
Make use of the following benefits:
§	Simplified access via easily usable Web Interface
§	Straight forward configuration on TPP server side
§	Automatic calculation of high-accurate coordinates 
§	Support of all commonly used GNSS system 
§	Results based on local reference station network
§	Automatic reporting via mail
§	Full support of TPP Accounting functionalities

For additional information on the new TOP App please refer to the Technical Notes that are available at http://www.trimble.com/infrastructure/.
If you are interested in the new Trimble Online Processing App please contact your Trimble sales representative. 

Trimble PivotTM Platform, version 3.5.3
Reference Data Shop
The zipping mechanism of the Reference Data Shop in advance of an order delivery has been revised for a smoother workflow.  

Ephemeris Storage
The storage of ephemeris information (RINEX format 3.02) for Galileo satellites has been improved.
This applies to both the Storage and Ephemeris Manager modules.

Ionosphere Activity Module
The check for the age of information coming from the GNSS receiver modules, the Atmosphere Watch modules and the Network Processor modules is more robust now and a warning message is shown if data are detected as too old.

RTX Engine
QZSS satellite processing support in the RTX Engine is now more stable. 

Network Processor (Sparse VRS)

The selection of a processing mode for an RTONet module has been realized now when inserting the module below a network processor that is running in sparse VRS mode.

Trimble PivotTM Platform, version 3.5.2
GNSS Receiver 
The verification of the tectonic plate selection has been reworked in connection with inserting a GNSS Receiver module and selecting a certain station that has previously been copied via the system properties. 

Atmosphere Watch 
Changes to the properties of an Atmosphere Watch module that is currently post processing is more stable now.

User Interface
The User Interface has been enhanced to reduce its response time and to run smoother on large systems consisting of several servers.

Trimble PivotTM Platform, version 3.5.1
RTO Net
The RTO Net module now includes an additional property setting that also allows accepting NMEA strings with 00:00:00 as time stamp.

Local Transformation
Local transformation within the RTO Net module is now shifting the coordinate of the closest physical base station (PBS) based on the transformation parameters. This applies to all formats including PBS messages. In addition, the robustness of Trimble Pivot Platform in conjunction with using local transformation has increased.
Azure Databases
Trimble Pivot Platform has been aligned to further warrant the interrelation with Microsoft® Azure™ databases. 

Master Setup
The Master Setup has been improved to make the loading process smoother and to reduce the response time. This is especially beneficial with lager systems.

Ntrip Caster
The mountpoint settings at the Ntrip Caster module properties have been updated and now make all the latest satellite navigation systems available for selection.

Synchronizer
Reloading the configuration on a distributed environment consisting of several servers has been enhanced. This has a positive impact especially on the interaction between the Synchronizer and associated modules like the RTK and RTX™ Engine. 

Weather Condition
The download logic of radiosonde data has been re-worked. The increased accuracy of download verification reduces the traffic on a system significantly.