Trimble 4D ControlTM Software, version 4.4.1
This software update for Trimble® 4D Control™ contains all changes since the release of version 4.4.0. The following document gives you an overview of the changes.

Data Collector/ Data Receiver

The alarm handling for terrestrial measurements from a Total Station to prisms has been revised. 
•	Alarm Evaluation Mode

A new Alarm Evaluation Mode setting at the properties of both modules allows determining in which shape an alarm is sent after a round measurement is finished.  An alarm is either sent only once covering all targets that met the alarm condition (Per Round) or several alarms are sent for each affected target (Per Target). 
•	Time Stamp

If an alarm condition is met during a round measurement it is ensured that the triggered alarm message shows proper time stamp information. 

T4D Web 

The translation of all available languages has been reworked and is now displayed in an easier and more comprehensive manner.  Translations for all supported languages are fully available and also apply to associated alarm messages.