Trimble PivotTM Platform, version 3.8.2
This software update for Trimble® Pivot™ Platform (TPP) contains all changes since the release of version 3.8.0. The following document gives you an overview of the changes.

Real-Time Output
Correction data output in CMRx format might have resulted in not letting rovers to fix. This issue exists in versions 3.8 and 3.8.1 (not in versions 3.5.8 and lower). This issue has been fixed with the software update 3.8.2.

Trimble PivotTM Platform, version 3.8.1
Network Processor
RTKNet
Network processing of QZSS signals failed in previous versions if BINEX was being used as GNSS observation data input format. This issue has been fixed.
RTXNet
The network processor's status view might have indicated a performance percentage higher than 100% (number of processed satellites in relation to number of solved satellites) while the number of solved satellites cannot be higher than the number of processed satellites. This potential issue has been fixed.

Local Transformation
In the unlikely event that the computation of local transformation parameters fails, transformation messages with values set to zero were sent out without further notification in previous versions. This software update introduces error messages in the Trimble Pivot Platform status view in case no transformation parameters can be provided while the user will be disconnected from the RTO (in case of RTO Net and multi-station RTO; in case of single-station RTO, the data stream will be stopped).

Trimble Ntrip Caster
0 bytes connections
Ntrip connections might hold connections with no data being sent without clearing these connections. This behavior could have resulted in a license limit exceeds or might have forced the Ntrip Caster to stop working. This potential issue has been resolved.
Mounpoint format data 
Trimble Ntrip Caster allows the creation of new mointpoints by copying existing mountpoints (parent). When using a copied mountpoint (child) and if the data format settings of the child get changed, the parent's data format settings get changed as well unintentionally, and vice-versa. This issue has been fixed.  

Storage
When using RTCM 3.2 MSM as GNSS observation data input format in Trimble Pivot Platform version 3.8, stored RINEX files have showed unrealistically high numbers of cycle slips. This issue has been resolved with this software update. 

Real-Time Output
The output of correction data in RTO Net with CMR+ format might have stopped and showed an error message in the status messages view in Trimble Pivot Platform version 3.8.0. This software update fixes this potential issue.

User Interface
Moving a large number of modules from one container to another might have resulted in no progress of the "Moving Modules" dialogue and in an unresponsive Trimble Pivot Platform User Interface. These potential issues have been resolved. A "Cancel" button has been added to the "Moving Modules" dialogue and the number of moved modules will be indicated. 

RTK Engine
Improved handling of CMRx input data. 

GNSS Receiver
IP Authentication
TCP/IP communication to Trimble NetRx GNSS receivers allows using IP authentication. The authentication password requires at least 7 characters. This requirement will be shown as information in the module information section with this software update. Once, a password of at least seven characters is set in Trimble Pivot Platform, the receiver connects as soon as the receiver's properties are adapted to the new password.