Trimble PivotTM Platform, version 3.5.2
This software update for Trimble® Pivot™ Platform (TPP) contains all changes since the release of version 3.5.0. The following document gives you an overview of the changes.

GNSS Receiver 
The verification of the tectonic plate selection has been reworked in connection with inserting a GNSS Receiver module and selecting a certain station that has previously been copied via the system properties. 

Atmosphere Watch 
Changes to the properties of an Atmosphere Watch module that is currently post processing is more stable now.

User Interface
The User Interface has been enhanced to reduce its response time and to run smoother on a large system consisting of several servers.

Trimble PivotTM Platform, version 3.5.1
RTO Net
The RTO Net module now includes an additional property setting that also allows accepting NMEA strings with 00:00:00 as time stamp.

Local Transformation

Local transformation within the RTO Net module is now shifting the coordinate of the closest physical base station (PBS) based on the transformation parameters. This applies to all formats including PBS messages. In addition, the robustness of Trimble Pivot Platform in conjunction with using local transformation has increased.
Azure Databases
Trimble Pivot Platform has been aligned to further warrant the interrelation with Microsoft® Azure™ databases. 

Master Setup

The Master Setup has been improved to make the loading process smoother and to reduce the response time. This is especially beneficial with lager systems.

Ntrip Caster
The mountpoint settings at the Ntrip Caster module properties have been updated and now make all the latest satellite navigation systems available for selection.

Synchronizer
Reloading the configuration on a distributed environment consisting of several servers has been enhanced. This has a positive impact especially on the interaction between the Synchronizer and associated modules like the RTK and RTX™ Engine. 

Weather Condition

The download logic of radiosonde data has been re-worked. The increased accuracy of download verification reduces the traffic on a system significantly.